| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

Macros
Commands Definitions
BLUENRG1 Peripheral Driver » FLASH Peripheral » Exported Constants

## Macros

#define | FLASH_ERASE 0x11
#define | FLASH_MASSERASE 0x22
#define | FLASH_WRITE 0x33
#define | FLASH_MASSWRITE 0x44
#define | FLASH_MASSREAD 0x55
#define | FLASH_SLEEP 0xAA
#define | FLASH_WAKEUP 0xBB
#define | FLASH_BURSTWRITE 0xCC
#define | IS_FLASH_CMD(CMD)

## Detailed Description

## Macro Definition Documentation

#define FLASH_BURSTWRITE 0xCC

Definition at line 112 of file BlueNRG1_flash.h.

#define FLASH_ERASE 0x11

Definition at line 105 of file BlueNRG1_flash.h.

#define FLASH_MASSERASE 0x22

Definition at line 106 of file BlueNRG1_flash.h.

#define FLASH_MASSREAD 0x55

Definition at line 109 of file BlueNRG1_flash.h.

#define FLASH_MASSWRITE 0x44

Definition at line 108 of file BlueNRG1_flash.h.

#define FLASH_SLEEP 0xAA

Definition at line 110 of file BlueNRG1_flash.h.

#define FLASH_WAKEUP 0xBB

Definition at line 111 of file BlueNRG1_flash.h.

#define FLASH_WRITE 0x33

Definition at line 107 of file BlueNRG1_flash.h.

#define IS_FLASH_CMD | ( |  | CMD | ) |

Value:
( ((CMD)==FLASH_ERASE) || ((CMD)==FLASH_MASSERASE) \
((CMD)==FLASH_WRITE) || ((CMD)==FLASH_MASSWRITE) \
((CMD)==FLASH_MASSREAD) || ((CMD)==FLASH_BURSTWRITE) \
((CMD)==FLASH_SLEEP) || ((CMD)==FLASH_WAKEUP) )
FLASH_WRITE
#define FLASH_WRITE
Definition: BlueNRG1_flash.h:107
FLASH_MASSREAD
#define FLASH_MASSREAD
Definition: BlueNRG1_flash.h:109
FLASH_MASSWRITE
#define FLASH_MASSWRITE
Definition: BlueNRG1_flash.h:108
FLASH_BURSTWRITE
#define FLASH_BURSTWRITE
Definition: BlueNRG1_flash.h:112
FLASH_ERASE
#define FLASH_ERASE
Definition: BlueNRG1_flash.h:105
FLASH_SLEEP
#define FLASH_SLEEP
Definition: BlueNRG1_flash.h:110
FLASH_WAKEUP
#define FLASH_WAKEUP
Definition: BlueNRG1_flash.h:111
FLASH_MASSERASE
#define FLASH_MASSERASE
Definition: BlueNRG1_flash.h:106

Definition at line 114 of file BlueNRG1_flash.h.