| STM32L - BlueNRG-1 BLE stack APIs, Events and Constants

- Main Page
- Modules
- Classes
- Files

- Class List
- Class Members

- All
- Variables

- a
- c
- d
- e
- f
- g
- h
- i
- l
- o
- p
- r
- s
- u

### - a -

- Address : Advertising_Report_t_s , Bonded_Device_Entry_t_s
- Address_Type : Advertising_Report_t_s , Bonded_Device_Entry_t_s

### - c -

- Char_UUID_128 : Char_Desc_Uuid_t_s , Char_UUID_t_s
- Char_UUID_16 : Char_Desc_Uuid_t_s , Char_UUID_t_s
- clen : hci_request
- Connection_Handle : Handle_Packets_Pair_Entry_t_s
- cparam : hci_request
- currentNode : _tHciDataPacket

### - d -

- Data : Advertising_Report_t_s
- data_len : _tHciDataPacket
- dataBuff : _tHciDataPacket

### - e -

- event : hci_request
- Event_Type : Advertising_Report_t_s

### - f -

- Found_Attribute_Handle : Attribute_Group_Handle_Pair_t_s

### - g -

- Group_End_Handle : Attribute_Group_Handle_Pair_t_s

### - h -

- Handle : Handle_Entry_t_s , Handle_Item_t_s
- HC_Num_Of_Completed_Packets : Handle_Packets_Pair_Entry_t_s

### - i -

- Include_UUID_128 : Include_UUID_t_s
- Include_UUID_16 : Include_UUID_t_s

### - l -

- Length_Data : Advertising_Report_t_s

### - o -

- ocf : hci_request
- ogf : hci_request

### - p -

- Peer_Address : Whitelist_Entry_t_s
- Peer_Address_Type : Whitelist_Entry_t_s

### - r -

- rlen : hci_request
- rparam : hci_request
- RSSI : Advertising_Report_t_s

### - s -

- Service_UUID_128 : Service_UUID_t_s
- Service_UUID_16 : Service_UUID_t_s

### - u -

- UUID_128 : UUID_t_s
- UUID_16 : UUID_t_s