| BlueNRG-1 ACI APIs and events callbacks

- Main Page
- Modules
- Classes
- Files

- Class List
- Class Members

- All
- Variables

- a
- b
- c
- d
- e
- f
- g
- h
- i
- l
- m
- n
- p
- r
- s
- u

Here is a list of all class members with links to the classes they belong to:

### - a -

- Address : Advertising_Report_t_s , Bonded_Device_Entry_t_s
- Address_Type : Advertising_Report_t_s , Bonded_Device_Entry_t_s
- attrValueArrSize : BlueNRG_Stack_Initialization_t

### - b -

- bleStartFlashAddress : BlueNRG_Stack_Initialization_t
- bleStartRamAddress : BlueNRG_Stack_Initialization_t

### - c -

- Char_UUID_128 : Char_Desc_Uuid_t_s , Char_UUID_t_s
- Char_UUID_16 : Char_Desc_Uuid_t_s , Char_UUID_t_s
- Connection_Handle : Handle_Packets_Pair_Entry_t_s

### - d -

- Data : Advertising_Report_t_s

### - e -

- Event_Type : Advertising_Report_t_s

### - f -

- Found_Attribute_Handle : Attribute_Group_Handle_Pair_t_s

### - g -

- Group_End_Handle : Attribute_Group_Handle_Pair_t_s

### - h -

- Handle : Handle_Entry_t_s , Handle_Item_t_s
- hardware_config : BlueNRG_Stack_Initialization_t
- HC_Num_Of_Completed_Packets : Handle_Packets_Pair_Entry_t_s
- hot_ana_config_table : hardware_config_table_t
- hs_startup_time : hardware_config_table_t

### - i -

- Include_UUID_128 : Include_UUID_t_s
- Include_UUID_16 : Include_UUID_t_s

### - l -

- Length_Data : Advertising_Report_t_s
- ls_source : hardware_config_table_t

### - m -

- master_sca : hardware_config_table_t
- max_conn_event_length : hardware_config_table_t

### - n -

- numAttrRecord : BlueNRG_Stack_Initialization_t
- numAttrServ : BlueNRG_Stack_Initialization_t
- numOfLinks : BlueNRG_Stack_Initialization_t

### - p -

- Peer_Address : Whitelist_Entry_t_s
- Peer_Address_Type : Whitelist_Entry_t_s

### - r -

- RSSI : Advertising_Report_t_s

### - s -

- secDbSize : BlueNRG_Stack_Initialization_t
- serverDbSize : BlueNRG_Stack_Initialization_t
- Service_UUID_128 : Service_UUID_t_s
- Service_UUID_16 : Service_UUID_t_s
- slave_sca : hardware_config_table_t
- stored_device_id_data_p : BlueNRG_Stack_Initialization_t

### - u -

- UUID_128 : UUID_t_s
- UUID_16 : UUID_t_s