| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

Macros
Conversion Mode Definitions
BLUENRG1 Peripheral Driver » ADC Peripheral » Exported Constants

## Macros

#define | ADC_ConversionMode_Single ((uint8_t)0x00)
#define | ADC_ConversionMode_Continuous ((uint8_t)0x08)
#define | IS_ADC_CONVERSIONMODE(CONVERSIONMODE)

## Detailed Description

## Macro Definition Documentation

#define ADC_ConversionMode_Continuous ((uint8_t)0x08)

Definition at line 126 of file BlueNRG1_adc.h.

#define ADC_ConversionMode_Single ((uint8_t)0x00)

Definition at line 125 of file BlueNRG1_adc.h.

#define IS_ADC_CONVERSIONMODE | ( |  | CONVERSIONMODE | ) |

Value:
(((CONVERSIONMODE) == ADC_ConversionMode_Single) || \
((CONVERSIONMODE) == ADC_ConversionMode_Continuous))
ADC_ConversionMode_Single
#define ADC_ConversionMode_Single
Definition: BlueNRG1_adc.h:125
ADC_ConversionMode_Continuous
#define ADC_ConversionMode_Continuous
Definition: BlueNRG1_adc.h:126

Definition at line 128 of file BlueNRG1_adc.h.