| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

Classes | Macros | Enumerations
Exported Types
BLUENRG1 Peripheral Driver » GPIO Peripheral

## Classes

struct | GPIO_InitType
| Structure definition of GPIO initialization. More...
struct | GPIO_EXTIConfigType
| Structure definition of GPIO EXTernal Interrupt initialization. More...

## Macros

#define | IS_GPIO_BIT_ACTION(ACTION) (((ACTION) == Bit_RESET) || ((ACTION) == Bit_SET))

## Enumerations

enum | BitAction { Bit_RESET = 0, Bit_SET }
| Bit_SET and Bit_RESET enumeration. More...

## Detailed Description

## Macro Definition Documentation

#define IS_GPIO_BIT_ACTION | ( |  | ACTION | ) | (((ACTION) == Bit_RESET) || ((ACTION) == Bit_SET))

This macro checks if ACTION is a valid bit action

Definition at line 94 of file BlueNRG1_gpio.h.

## Enumeration Type Documentation

enum BitAction

Bit_SET and Bit_RESET enumeration.

Enumerator
Bit_RESET | Specifies the GPIO reset state
Bit_SET | Specifies the GPIO set state

Definition at line 87 of file BlueNRG1_gpio.h.