| BlueNRG-1 SDK drivers APIs

- Main Page
- Modules
- Classes
- Files

Macros
LSM6DS3_XG_Gyroscope_Full_Scale_Selection_CTRL2_G
SDK EVAL BlueNRG1 » LSM6DS3 » LSM6DS3 SENSOR LIB » LSM6DS3_Exported_Defines

## Macros

#define | LSM6DS3_G_FS_125_DISABLE ((uint8_t)0x00)
#define | LSM6DS3_G_FS_125_ENABLE ((uint8_t)0x02)
#define | LSM6DS3_G_FS_125_MASK ((uint8_t)0x02)
#define | LSM6DS3_G_FS_245 ((uint8_t)0x00)
#define | LSM6DS3_G_FS_500 ((uint8_t)0x04)
#define | LSM6DS3_G_FS_1000 ((uint8_t)0x08)
#define | LSM6DS3_G_FS_2000 ((uint8_t)0x0C)
#define | LSM6DS3_G_FS_MASK ((uint8_t)0x0C)

## Detailed Description

## Macro Definition Documentation

#define LSM6DS3_G_FS_1000 ((uint8_t)0x08)

Full scale: 1000 dps

Definition at line 1099 of file lsm6ds3.h.

#define LSM6DS3_G_FS_125_DISABLE ((uint8_t)0x00)

Full scale: 125 dps enable: disable

Definition at line 1092 of file lsm6ds3.h.

#define LSM6DS3_G_FS_125_ENABLE ((uint8_t)0x02)

Full scale: 125 dps enable: enable

Definition at line 1093 of file lsm6ds3.h.

#define LSM6DS3_G_FS_125_MASK ((uint8_t)0x02)

Definition at line 1095 of file lsm6ds3.h.

#define LSM6DS3_G_FS_2000 ((uint8_t)0x0C)

Full scale: 2000 dps

Definition at line 1100 of file lsm6ds3.h.

#define LSM6DS3_G_FS_245 ((uint8_t)0x00)

Full scale: 245 dps

Definition at line 1097 of file lsm6ds3.h.

#define LSM6DS3_G_FS_500 ((uint8_t)0x04)

Full scale: 500 dps

Definition at line 1098 of file lsm6ds3.h.

#define LSM6DS3_G_FS_MASK ((uint8_t)0x0C)

Definition at line 1102 of file lsm6ds3.h.