| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

- Class List
- Class Members

Public Attributes | List of all members
ADC_InitType Struct Reference
BLUENRG1 Peripheral Driver » ADC Peripheral » Exported Types

Structure definition of ADC initialization. More...

`#include <BlueNRG1_adc.h>`

## Public Attributes

uint8_t | ADC_DecimationRate
uint8_t | ADC_Input
uint8_t | ADC_ConversionMode
uint8_t | ADC_Attenuation
uint8_t | ADC_ReferenceVoltage

## Detailed Description

Structure definition of ADC initialization.

Definition at line 49 of file BlueNRG1_adc.h.

## Member Data Documentation

uint8_t ADC_InitType::ADC_Attenuation

Specifies the attenuation. This parameter can be a value of ADC_Attenuation

Definition at line 59 of file BlueNRG1_adc.h.

uint8_t ADC_InitType::ADC_ConversionMode

Specifies the conversion mode. This parameter can be a value of ADC_ConversionMode

Definition at line 56 of file BlueNRG1_adc.h.

uint8_t ADC_InitType::ADC_DecimationRate

Specifies the decimation rate. This parameter can be a value of ADC_DecimationRate

Definition at line 50 of file BlueNRG1_adc.h.

uint8_t ADC_InitType::ADC_Input

Specifies the input used for the conversion. This parameter can be a value of ADC_Input

Definition at line 53 of file BlueNRG1_adc.h.

uint8_t ADC_InitType::ADC_ReferenceVoltage

Specifies the ADC reference voltage. This parameter can be a value of ADC_ReferenceVoltage

Definition at line 62 of file BlueNRG1_adc.h.

The documentation for this struct was generated from the following file:

- BlueNRG1_adc.h