| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

Macros
Peripherals Clock
BLUENRG1 Peripheral Driver » System Control » Exported Constants

## Macros

#define | CLOCK_PERIPH_GPIO ((uint32_t)0x00000001)
#define | CLOCK_PERIPH_NVM ((uint32_t)0x00000002)
#define | CLOCK_PERIPH_SYS_CONTROL ((uint32_t)0x00000004)
#define | CLOCK_PERIPH_UART ((uint32_t)0x00000008)
#define | CLOCK_PERIPH_SPI ((uint32_t)0x00000010)
#define | CLOCK_PERIPH_WDG ((uint32_t)0x00000080)
#define | CLOCK_PERIPH_ADC ((uint32_t)0x00000100)
#define | CLOCK_PERIPH_I2C1 ((uint32_t)0x00000200)
#define | CLOCK_PERIPH_I2C2 ((uint32_t)0x00000400)
#define | CLOCK_PERIPH_MTFX1 ((uint32_t)0x00000800)
#define | CLOCK_PERIPH_MTFX2 ((uint32_t)0x00001000)
#define | CLOCK_PERIPH_RTC ((uint32_t)0x00002000)
#define | CLOCK_PERIPH_DMA ((uint32_t)0x00010000)
#define | CLOCK_PERIPH_RNG ((uint32_t)0x00020000)
#define | IS_CLOCK_PERIPH(PERIPH) ((PERIPH & 0x00033F9F) != 0)

## Detailed Description

## Macro Definition Documentation

#define CLOCK_PERIPH_ADC ((uint32_t)0x00000100)

Definition at line 85 of file BlueNRG1_sysCtrl.h.

#define CLOCK_PERIPH_DMA ((uint32_t)0x00010000)

Definition at line 91 of file BlueNRG1_sysCtrl.h.

#define CLOCK_PERIPH_GPIO ((uint32_t)0x00000001)

Definition at line 79 of file BlueNRG1_sysCtrl.h.

#define CLOCK_PERIPH_I2C1 ((uint32_t)0x00000200)

Definition at line 86 of file BlueNRG1_sysCtrl.h.

#define CLOCK_PERIPH_I2C2 ((uint32_t)0x00000400)

Definition at line 87 of file BlueNRG1_sysCtrl.h.

#define CLOCK_PERIPH_MTFX1 ((uint32_t)0x00000800)

Definition at line 88 of file BlueNRG1_sysCtrl.h.

#define CLOCK_PERIPH_MTFX2 ((uint32_t)0x00001000)

Definition at line 89 of file BlueNRG1_sysCtrl.h.

#define CLOCK_PERIPH_NVM ((uint32_t)0x00000002)

Definition at line 80 of file BlueNRG1_sysCtrl.h.

#define CLOCK_PERIPH_RNG ((uint32_t)0x00020000)

Definition at line 92 of file BlueNRG1_sysCtrl.h.

#define CLOCK_PERIPH_RTC ((uint32_t)0x00002000)

Definition at line 90 of file BlueNRG1_sysCtrl.h.

#define CLOCK_PERIPH_SPI ((uint32_t)0x00000010)

Definition at line 83 of file BlueNRG1_sysCtrl.h.

#define CLOCK_PERIPH_SYS_CONTROL ((uint32_t)0x00000004)

Definition at line 81 of file BlueNRG1_sysCtrl.h.

#define CLOCK_PERIPH_UART ((uint32_t)0x00000008)

Definition at line 82 of file BlueNRG1_sysCtrl.h.

#define CLOCK_PERIPH_WDG ((uint32_t)0x00000080)

Definition at line 84 of file BlueNRG1_sysCtrl.h.

#define IS_CLOCK_PERIPH | ( |  | PERIPH | ) | ((PERIPH & 0x00033F9F) != 0)

Definition at line 94 of file BlueNRG1_sysCtrl.h.