| BlueNRG-1 DK: BLE examples

- Main Page
- Modules
- Files

- File List

File List
Here is a list of all files with brief descriptions:
[detail level 1 2]

▼ BLE_Throughput |
BLE_Throughput_main.c | This is a Throughput demo that shows how to implement a simple throughput test between two BlueNRG-1 devices. Two throughput test options are available: unidirectional (server notification to client side); bidirectional (server notification to client side and write without response from client to server side)
▼ DTM |
DTM_main.c | This application configures a BlueNRG-1 device as a network coprocessor (SPI or UART) in order to be used with the BlueNRG GUI or other instruments as CBT
BLE_ANCS_main.c | This is a BLE ANCS demo that shows how to configure a BlueNRG-1 device in order to works like a notification consumer device
BLE_Beacon_main.c | This is a BLE beacon demo that shows how to configure a BlueNRG-1 device in order to advertise specific manufacturing data and allow another BLE device to know if it is in the range of the BlueNRG-1 beacon device. It also provides a reference example about how using the BLE Over-The-Air (OTA) Service Manager firmware upgrade capability
BLE_Chat_main.c | This is a Chat demo that shows how to implement a simple 2-way communication between two BlueNRG-1 devices. It also provides a reference example about how using the BLE Over-The-Air (OTA) firmware upgrade capability with the BLE Chat Demo
BLE_Chat_Master_Slave_main.c | This is a Chat demo that shows how to implement a simple 2-way communication between only two BlueNRG-1 devices (single application for both devices)
main.c | This application contains an example which shows how implementing a device that uses the standard HID/HOGP Bluetooth Low Energy application profile. The device implemented to demo are keyboard and mouse
OTA_ResetManager_main.c | This application implements the OTA Reset Manager which, at reset, passes control to the latest valid BLE application updated through the BLE Over-The-Air (OTA) Service
OTA_ServiceManager_main.c | This application implements a basic standalone BLE Over The Air (OTA) firmware updgrade. It provides the BLE Over-The-Air Service management for handling the OTA firmware upgrade of a BlueNRG-1 application which doesn't have any BLE OTA service
BLE_RC_main.c | This example shows a simple remote control application (like an attuator)
SensorDemo_main.c | This application contains an example which shows how implementing a proprietary Bluetooth Low Energy profile: the sensor profile. It also provides a reference example about how using the BLE Over-The-Air (OTA) firmware upgrade capability with the BLE Sensor Demo
SensorDemo_central_role_main.c | This application implements a basic version of the BlueNRG-1 Sensor Profile Central role which emulates the BlueNRG-1 Sensor Demo applications available for smartphones (iOS and android)