| BlueNRG-1 Master/Central Library

- Main Page
- Classes
- Files

- Class List
- Class Members

Public Attributes | List of all members
securitySetS Struct Reference

Master security parameter settings. More...

`#include <master_basic_profile.h>`

## Public Attributes

uint8_t | ioCapability
uint8_t | mitm_mode
uint8_t | oob_enable
uint8_t | oob_data [16]
uint8_t | bonding_mode
uint8_t | use_fixed_pin
uint32_t | fixed_pin

## Detailed Description

Master security parameter settings.

Definition at line 288 of file master_basic_profile.h.

## Member Data Documentation

uint8_t securitySetS::bonding_mode

Bonding Mode flag

Definition at line 298 of file master_basic_profile.h.

uint32_t securitySetS::fixed_pin

Fixed pin to be used during pairing if MIMT protection is enabled. Any random value between 0 to 999999

Definition at line 305 of file master_basic_profile.h.

uint8_t securitySetS::ioCapability

Set the IO capabilities of the device.

Definition at line 290 of file master_basic_profile.h.

uint8_t securitySetS::mitm_mode

Man in the middle mode

Definition at line 292 of file master_basic_profile.h.

uint8_t securitySetS::oob_data[16]

Out of Band data

Definition at line 296 of file master_basic_profile.h.

uint8_t securitySetS::oob_enable

Out of Band authentication enabled

Definition at line 294 of file master_basic_profile.h.

uint8_t securitySetS::use_fixed_pin

Use fixed pin during pairing process

Definition at line 300 of file master_basic_profile.h.

The documentation for this struct was generated from the following file:

- master_basic_profile.h