| BlueNRG-1 SDK drivers APIs

- Main Page
- Modules
- Classes
- Files

Variables
LPS25HB_Private_Variables
SDK EVAL BlueNRG1 » LPS25HB » LPS25HB SENSOR LIB

## Variables

PRESSURE_DrvTypeDef | LPS25HBDrv
uint8_t | LPS25HB_SlaveAddress = LPS25HB_ADDRESS_LOW

## Detailed Description

## Variable Documentation

uint8_t LPS25HB_SlaveAddress = LPS25HB_ADDRESS_LOW

Definition at line 93 of file LPS25HB.c.

PRESSURE_DrvTypeDef LPS25HBDrv

Initial value:
=
{
LPS25HB_Init,
LPS25HB_PowerOff,
LPS25HB_ReadID,
LPS25HB_RebootCmd,
0,
0,
0,
0,
0,
LPS25HB_GetPressure,
LPS25HB_GetTemperature,
LPS25HB_SlaveAddrRemap,
NULL
}
NULL
#define NULL
Definition: LPS25HB.h:68

Definition at line 67 of file LPS25HB.c.