| BlueNRG-1 Master/Central Library

- Main Page
- Classes
- Files

- Class List
- Class Members

Public Attributes | List of all members
initDevS Struct Reference

Master initialization parameters. More...

`#include <master_basic_profile.h>`

## Public Attributes

uint8_t | public_addr [6]
uint8_t | device_name_len
uint8_t * | device_name
uint8_t | txPowerLevel

## Detailed Description

Master initialization parameters.

Definition at line 263 of file master_basic_profile.h.

## Member Data Documentation

uint8_t* initDevS::device_name

Device name to configure.

Definition at line 270 of file master_basic_profile.h.

uint8_t initDevS::device_name_len

Length of the device name. If the length is equal to zero the device name is ignored. For the BlueNRG-MS the device name length can be grater than 8.

Definition at line 268 of file master_basic_profile.h.

uint8_t initDevS::public_addr[6]

Public address

Definition at line 265 of file master_basic_profile.h.

uint8_t initDevS::txPowerLevel

Transmit power level Possible value are: 0 = -14 dBm, 1 = -11 dBm, 2 = -8 dBm, 3 = -5 dBm, 4 = -2 dBm, 5 = 2 dBm, 6 = 4 dBm, 7 = 8 dBm

Definition at line 282 of file master_basic_profile.h.

The documentation for this struct was generated from the following file:

- master_basic_profile.h