| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

- Class List
- Class Members

Public Attributes | List of all members
RTC_DateTimeType Struct Reference
BLUENRG1 Peripheral Driver » RTC Peripheral » Exported Types

Structure definition of RTC DateTime. More...

`#include <BlueNRG1_rtc.h>`

## Public Attributes

uint8_t | Second
uint8_t | Minute
uint8_t | Hour
uint8_t | WeekDay
uint8_t | MonthDay
uint8_t | Month
uint16_t | Year

## Detailed Description

Structure definition of RTC DateTime.

Definition at line 80 of file BlueNRG1_rtc.h.

## Member Data Documentation

uint8_t RTC_DateTimeType::Hour

Specify the present hour to be set to RTC clockwatch. This parameter can be integer value in range from 0 to 23

Definition at line 88 of file BlueNRG1_rtc.h.

uint8_t RTC_DateTimeType::Minute

Specify the present minute to be set to RTC clockwatch. This parameter can be integer value in range from 0 to 59

Definition at line 85 of file BlueNRG1_rtc.h.

uint8_t RTC_DateTimeType::Month

Specify the present month to be set to RTC clockwatch. This parameter can be an integer value in range from 1 to 12 (depends on month)

Definition at line 97 of file BlueNRG1_rtc.h.

uint8_t RTC_DateTimeType::MonthDay

Specify the present day in the month to be set to RTC clockwatch. This parameter can be an integer value in range from 1 to 31 (depends on month)

Definition at line 94 of file BlueNRG1_rtc.h.

uint8_t RTC_DateTimeType::Second

Specify the present second to be set to RTC clockwatch. This parameter can be integer value in range from 0 to 59

Definition at line 82 of file BlueNRG1_rtc.h.

uint8_t RTC_DateTimeType::WeekDay

Specify the present day in the week to be set to RTC clockwatch. This parameter can be an integer value in range from 0 to 7

Definition at line 91 of file BlueNRG1_rtc.h.

uint16_t RTC_DateTimeType::Year

Specify the present year to be set to RTC clockwatch. This parameter can be an integer value in range from 0 to 3999 (depends on month)

Definition at line 100 of file BlueNRG1_rtc.h.

The documentation for this struct was generated from the following file:

- BlueNRG1_rtc.h