| STM32L - BlueNRG-1 BLE stack APIs, Events and Constants

- Main Page
- Modules
- Classes
- Files

- Class List
- Class Members

Public Attributes | List of all members
Handle_Packets_Pair_Entry_t_s Struct Reference
HCI events

`#include <bluenrg1_events.h>`

## Public Attributes

uint16_t | Connection_Handle
uint16_t | HC_Num_Of_Completed_Packets

## Detailed Description

Documentation for Handle_Packets_Pair_Entry_t

Definition at line 35 of file bluenrg1_events.h.

## Member Data Documentation

uint16_t Handle_Packets_Pair_Entry_t_s::Connection_Handle

Connection_Handle

Definition at line 36 of file bluenrg1_events.h.

uint16_t Handle_Packets_Pair_Entry_t_s::HC_Num_Of_Completed_Packets

The number of HCI Data Packets that have been completed (transmitted or flushed) for the associated Connection_Handle since the previous time the event was returned. Range for N: 0x0000-0xFFFF

Definition at line 40 of file bluenrg1_events.h.

The documentation for this struct was generated from the following file:

- bluenrg1_events.h