| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

Macros
Own address
BLUENRG1 Peripheral Driver » I2C Peripheral » Exported Constants

## Macros

#define | IS_I2C_OWN_ADDRESS1(ADDRESS1) ((ADDRESS1) <= 0x3FF)
#define | IS_I2C_OWN_ADDRESS(ADDRESS2) ((ADDRESS2) <= 0x7F)

## Detailed Description

## Macro Definition Documentation

#define IS_I2C_OWN_ADDRESS | ( |  | ADDRESS2 | ) | ((ADDRESS2) <= 0x7F)

This macro checks if ADDRESS2 is a valid address value

Definition at line 278 of file BlueNRG1_i2c.h.

#define IS_I2C_OWN_ADDRESS1 | ( |  | ADDRESS1 | ) | ((ADDRESS1) <= 0x3FF)

This macro checks if ADDRESS1 is a valid address value

Definition at line 274 of file BlueNRG1_i2c.h.