| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

Enumerations
Exported Types
BLUENRG1 Peripheral Driver » System Control

## Enumerations

enum | RESET_REASON_Type { RESET_NONE, RESET_SYSREQ, RESET_WDG, RESET_LOCKUP, RESET_BLE_BOR, RESET_BLE_POR, RESET_BLE_WAKEUP_FROM_IO9, RESET_BLE_WAKEUP_FROM_IO10, RESET_BLE_WAKEUP_FROM_IO11, RESET_BLE_WAKEUP_FROM_IO12, RESET_BLE_WAKEUP_FROM_IO13, RESET_BLE_WAKEUP_FROM_TIMER1,
RESET_BLE_WAKEUP_FROM_TIMER2
}
| System Reset and Wakeup Sources. More...

## Detailed Description

## Enumeration Type Documentation

enum RESET_REASON_Type

System Reset and Wakeup Sources.

Enumerator
RESET_NONE |
RESET_SYSREQ |
RESET_WDG |
RESET_LOCKUP |
RESET_BLE_BOR |
RESET_BLE_POR |
RESET_BLE_WAKEUP_FROM_IO9 |
RESET_BLE_WAKEUP_FROM_IO10 |
RESET_BLE_WAKEUP_FROM_IO11 |
RESET_BLE_WAKEUP_FROM_IO12 |
RESET_BLE_WAKEUP_FROM_IO13 |
RESET_BLE_WAKEUP_FROM_TIMER1 |
RESET_BLE_WAKEUP_FROM_TIMER2 |

Definition at line 50 of file BlueNRG1_sysCtrl.h.