| BlueNRG-1 Master/Central Library

- Main Page
- Classes
- Files

- Class List
- Class Members

Public Attributes | List of all members
connUpdateParamS Struct Reference

Connection Parameters received from peer peripheral device during an l2cap connection parameter update request. More...

`#include <master_basic_profile.h>`

## Public Attributes

uint8_t | identifier
uint16_t | interval_min
uint16_t | interval_max
uint16_t | slave_latency
uint16_t | timeout_mult
uint16_t | min_conn_length
uint16_t | max_conn_length

## Detailed Description

Connection Parameters received from peer peripheral device during an l2cap connection parameter update request.

Definition at line 421 of file master_basic_profile.h.

## Member Data Documentation

uint8_t connUpdateParamS::identifier

This is the identifier which associates the request to the response. The same identifier has to be returned by the upper layer in the command Master_ConnectionUpdateParamResponse().

Definition at line 426 of file master_basic_profile.h.

uint16_t connUpdateParamS::interval_max

Maximum value for the connection event interval. This shall be greater than or equal to interval_min.
Range: 0x0006 to 0x0C80
Time = N x 1.25 msec
Time Range: 7.5 msec to 4 seconds

Definition at line 440 of file master_basic_profile.h.

uint16_t connUpdateParamS::interval_min

Minimum value for the connection event interval. This shall be less than or equal to interval_max.
Range: 0x0006 to 0x0C80
Time = N x 1.25 msec
Time Range: 7.5 msec to 4 seconds

Definition at line 433 of file master_basic_profile.h.

uint16_t connUpdateParamS::max_conn_length

Maximum length of connection needed for the LE connection.
Range: 0x0000 - 0xFFFF
Time = N x 0.625 msec.

Definition at line 460 of file master_basic_profile.h.

uint16_t connUpdateParamS::min_conn_length

Minimum length of connection needed for the LE connection.
Range: 0x0000 - 0xFFFF
Time = N x 0.625 msec.

Definition at line 455 of file master_basic_profile.h.

uint16_t connUpdateParamS::slave_latency

Slave latency for the connection in number of connection events.
Range: 0x0000 to 0x01F4

Definition at line 444 of file master_basic_profile.h.

uint16_t connUpdateParamS::timeout_mult

Supervision timeout for the LE Link.
Range: 0x000A to 0x0C80
Time = N x 10 msec
Time Range: 100 msec to 32 seconds

Definition at line 450 of file master_basic_profile.h.

The documentation for this struct was generated from the following file:

- master_basic_profile.h