| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

- File List
- File Members

Functions
BlueNRG1_rtc.c File Reference

This file provides all the RTC firmware functions. More...

`#include "BlueNRG1_rtc.h"`

Go to the source code of this file.

## Functions

void | RTC_Init (RTC_InitType *RTC_InitStruct)
| Initializes the RTC peripheral according to the specified parameters in the RTC_InitStruct. More...
void | RTC_Cmd (FunctionalState NewState)
| Enables or disables selected RTC peripheral. More...
void | RTC_IT_Config (uint8_t RTC_IT, FunctionalState NewState)
| Enables or disables selected RTC interrupt. More...
ITStatus | RTC_IT_Status (uint8_t RTC_IT)
| Return the RTC interrupt status for the specified IT. More...
void | RTC_IT_Clear (uint8_t RTC_IT)
| Clear selected RTC interrupt. More...
void | RTC_ClockwatchCmd (FunctionalState NewState)
| Enables or disables selected RTC clockwatch. More...
void | RTC_SetTimeDate (RTC_DateTimeType *RTC_DateTime)
| Initialize the RTC clockwatch with present time and date. More...
void | RTC_SetMatchTimeDate (RTC_DateTimeType *RTC_MatchDataTime)
| Set the RTC clockwatch match date and time registers. More...
void | RTC_GetTimeDate (RTC_DateTimeType *RTC_DataTime)
| Set the RTC clockwatch match date and time registers. More...
uint32_t | RTC_GetTimerValue (void)
| Return the actual timer counter. More...
uint32_t | RTC_GetNumberIrqGenerated (void)
| Return the actual number of interrupt generated by RTC. More...
void | RTC_AutoStart (FunctionalState NewState)
| Enables or disables the auto start on load register or pattern register write operation. More...
void | RTC_SelectTrimmedClock (FunctionalState NewState)
| Enables or disables the use of the trimmed 32 kHz clock. More...

## Detailed Description

This file provides all the RTC firmware functions.

Author
  VMA Application Team

Version
  V2.0.0

Date
  21-March-2016

Attention

THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE TIME. AS A RESULT, STMICROELECTRONICS SHALL NOT BE HELD LIABLE FOR ANY DIRECT, INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM THE CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE CODING INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.

##
© COPYRIGHT 2016 STMicroelectronics

Definition in file BlueNRG1_rtc.c.